( TL19E00H46400027195KBAT00 )

Front Impact Sensor Replacement

Installation

1. Install the front impact sensor with a new TORX bolts (A), then connect the left or right engine compartment wire harness 2P connector (B) to the front impact sensor (C).

1. Reconnect the driver's airbag 4P connector, the front passenger's airbag 4P connector, both seat belt tensioner 4P connectors, and both seat belt outer lap tensioner 2P connectors.

1. Do the battery terminal reconnection procedure.

1. Confirm proper SRS operation: Turn the ignition switch to ON (II); the SRS indicator should come on for about 6 seconds and then go off.

1. Reinstall all removed parts.