( TL19E10K791000R119XFAAT00 )

DTC Troubleshooting: 11-9x

DTC 11-9x (‘‘x'' can be 0 thru 9 or A thru F):
Short to Ground in the Driver's Airbag First Inflator (LHD model)
NOTE:

- Before doing this troubleshooting procedure, review SRS Precautions and Procedures and General Troubleshooting Information.
- Before replacing the SRS unit, check the SRS unit software version with the HDS. If the software version is not the latest, update the SRS unit software and retest.

1. Clear the DTC memory.

1. Turn the ignition switch to ON (II), then wait for 10 seconds.

1. Read the DTC.

Is DTC 11-9x indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.

1. Turn the ignition switch to LOCK (0).

1. Do the battery terminal disconnection procedure , then wait for 3 minutes.

1. Disconnect SRS unit connector A (39P) from the SRS unit.

1. Connect an SRS short canceller (070AZ-SAA0100) to the No. 3 and the No. 4 terminals of the SRS unit connector A (39P).

1. Check for continuity between the No. 3 and the No. 4 terminals of SRS unit connector A (39P) and body ground.

Is there continuity?

YES | - | Go to Step 9 .
NO | - | Faulty SRS unit; replace the SRS unit. ■

1. Disconnect the driver's airbag 4P connector from the cable reel.