( TL19E00J32300027157KBAT00 )

Footwell Light Replacement

Driver's

1. Remove the driver's dashboard undercover.

1. Disconnect the 2P connector (A) from the driver's footwell light (B).

1. Remove the footwell light.

1. Install the light in the reverse order of removal.

Passenger's

1. Remove the passenger's dashboard undercover.

1. Disconnect the 2P connector (A) from the passenger's footwell light (B).

1. Remove the footwell light.

1. Install the light in the reverse order of removal.