( TL19E00000000000000JCAT32 )

Maintenance Schedule for Severe Conditions - South Africa
60,000km(4year)

Follow the severe conditions maintenance schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km per trip or, in freezing temperatures, driving less than 16 km per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go driving.
- Towing trailer, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the vehicle is driven OCCASIONALLY under severe conditions, follow the normal conditions maintenance schedule.
Service at the indicated distance or time whichever comes first

| Replace engine oil filter R20A3, K24Z3

| Replace Manual Transmission Fluid

Use genuine Honda MTF.

| Replace Automatic Transmission Fluid

Use genuine Honda ATF-Z1.
Replace 60,000 km or 4 years, then every 45,000 km or 3 years

| Check parking brake adjustment

Check the parking brake operation.

| Replace dust and pollen filter

When the vehicle is drive mostly in areas that have high concentrations of dust, pollen, or soot in the air, replace the filter whenever airflow from the heating

| Brake hoses and lines (including VSA lines)

Check the master cylinder and VSA modulator-control unit and leakage.

| All fluid levels and condition of fluids

Check levels and check for leaks. If necessary, add.

|  | Engine coolant R20A3, K24Z3
|  | MTF
|  | ATF
|  | Brake fluid
|  | Clutch fluid
|  | Windshield washer fluid

| Exhaust system R20A3, K24Z3 Check the exhaust pipe and muffler for damage, leaks, and tightness.

| Fuel lines R20A3, K24Z3

and connections R20A3, K24Z3

|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damaged parts.

Every 7,500 km

| Replace engine oil R20A3, K24Z3

Every 15,000 km

| Replace air cleaner element R20A3, K24Z3

| Rotate tyres

Check tyre inflation and condition at least once per month.

Every 45,000 km

| Inspect valve clearance R20A3, K24Z3

Every 105,000 km

| Replace spark plugs R20A3, K24Z3

At 200,000 km or 10 years, then every 100,000 km or 5 years

| Replace engine coolant R20A3, K24Z3

Use genuine Honda All Season Antifreeze/Coolant Type 2.

Every 7,500 km or 6 months

| Check front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks.
|  | Check the calipers for damage, leaks, and tightness.

| Tie-rod ends, steering gearbox, and boots

|  | Check rack grease and steering linkage.
|  | Check the boot for damage and leaking grease.

| Suspension components

|  | Check the bolts for tightness.
|  | Check all dust cover for deterioration and damage.

| Driveshaft boots

|  | Check the boot and boot band for cracks.
|  | Check rack grease.

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check the brake fluid level between upper and lower marks on the reservoir.