( TL19E00J16126720801KBAT00 )

Front Door Latch Replacement

With Super Locking
NOTE: Put on gloves to protect your hands.

1. Remove these items:
   - Tweeter cover
   - Door panel
   - Inner handle
   - Door end trim

1. Raise the glass fully.

1. Remove the plastic cover as needed.

1. Detach the rod fastener, and disconnect the outer handle rod from the outer handle base.

1. Driver's door: While holding the outer handle cover from outside of the door, loosen the bolt until it can be pulled out half-way by hand, and then release the hooks of the outer handle cover, then remove the cover.

1. Driver's door: Release the hooks, then remove the lock cylinder from the outer handle base.

1. Pull the glass run channel (A) away as needed, and remove the bolt, then remove the center lower channel (B) by pulling it downward.