( TL19E00J18533231801KBAT00 )

Hood Latch Replacement

1. Install the latch in the reverse order of removal, and note these items:
   - Apply multipurpose grease to each location of the hood latch indicated by the arrows.
   - Make sure the hood opener cable is connected properly and hood latch switch connector is plugged in properly (for some models).
   - Adjust the hood latch alignment.
   - Make sure the hood opens properly and locks securely.