( TL19E1AE34150200000LDAT00 )

M/T Countershaft Reassembly

Exploded View
Special Tools Required
Inner driver handle, 40 mm
07746-0030100
Inner bearing driver attachment, 30 mm
07746-0030300
NOTE: Refer to the Exploded View, as needed, during this procedure.

1. Clean all parts in solvent, dry them, and apply MTF to all contact surfaces.

1. Install the 1st gear distance collar (A) with the needle bearing (B) and the 1st gear (C) onto the countershaft (D).