( TL19E20A18223800000KCAT00 )

Engine Installation

1. Install the transmission mount (A), then tighten the new transmission mount mounting bolts in the numbered sequence shown.

1. Install the ground cables (B).

1. Raise the vehicle on the lift to full height.

1. Install a new set ring on the end of each driveshaft, then install the driveshafts. Make sure each ring ‘‘clicks'' into place in the differential and the intermediate shaft.

1. Connect the lower arms to the knuckles.

1. Install the damper fork.

1. A/T model: Install the shift cable.

M/T model
A/T model