( TL19E00J46643421011FEAT00 )

Door Lock Knob Switch Test

Rear Door with Security

1. Remove the left or right rear door panel.

1. Disconnect the 10P connector (A) from the actuator (B).
   NOTE: The illustration shows the left rear door.

1. Check for continuity between the terminals.
   There should be continuity between the No. 7 [No. 8] and No. 5 [No. 10] terminals when the door lock knob switch is UNLOCK position and no continuity when the switch is in the LOCK position.
   [ ]: Right rear door

1. If the continuity is not as specified, replace the door lock actuator.