( TL19E00J36100000000CAAT20 )

Interface Dial Inputs and Outputs
Interface Dial 5P Connector

Terminal Number | Wire Color | Terminal Name | Description | Voltage (about) | Symptom
--- | --- | --- | --- | --- | ---
1 | WHT | JOG (jog) | Interface dial operation signal | 0−5 V pulses | If open: You can not operate navigation system. If short to ground: You can not operate navigation system.
2 | BLK * | SH JOG (Shield jog) | Shield for interface dial signal | ——— | ———
3 | BLK | GND (Ground) (G401) | Ground for interface dial | 0 V | If open: You can not operate navigation system. If short to ground: No effect on operation.
4 | PUR | ACC (Accessory) | Power source for interface dial | Battery voltage at ACC (I) | If open: You can not operate navigation system. If short to ground: Blows fuse No. 18 (7.5 A) in the driver's under-dash fuse/relay box.

*: | The shielded wires have a heat-shrink tube insulating the outside of the wire. The color of the insulating tube, typically black or dark gray, may not match the color of the wire shown on the circuit diagram.