( TL19E30A20323400000FAAT00 )

EVAP System Troubleshooting

Special Tools Required
Combination gauge kit 20/−100 kPa
07YAJ-0010610
Tube joint adapter
07410-5790503

1. Disconnect the vacuum hose (A) from the EVAP canister (B) and connect a vacuum pump/gauge (C) to the hose.

1. Start the engine, and let it idle.
   NOTE: Engine coolant temperature must be below 55 °C (131 °F).

Is there vacuum?

YES | - | Inspect vacuum hose routing. If OK, replace the EVAP canister purge valve. ■
NO | - | Go to Step 3 .

1. Hold the engine speed at 3,000 rpm (min −1 ) without load (A/T in N or P, M/T in neutral) until the radiator fan comes on, then hold the engine speed to 3,000 rpm (min −1 ).

Is there vacuum?

YES | - | Go to Step 4 .
NO | - | Inspect vacuum hose routing. If OK, replace the EVAP canister purge valve. ■

1. Turn the ignition switch to LOCK (0).

1. Reconnect the vacuum hose to the EVAP canister.

1. Remove the fuel fill cap.

1. Disconnect the purge air hose (A) from the EVAP canister and connect the combination gauge kit and tube joint adapter to EVAP canister (B).

1. Start the engine, and raise speed to 3,000 rpm (min −1 ).

Does vacuum appear on gauge within 1 minute?

YES | - | See EVAP two way valve test to complete. Evaporative emission controls are OK.■
NO | - | Replace the EVAP canister. ■