( TL19E1AE34150439533KBAT00 )

M/T Clutch Housing Mainshaft Bearing and Oil Seal Replacement

Special Tools Required
Oil seal driver, 65 mm
07JAD-PL90100
Adjustable bearing puller, 20−40 mm
07JAC-PH80100
Bearing remover shaft
07JAC-PH80200
Bearing driver attachment, 42 x 47 mm
07746-0010300
Driver handle, 15 x 135L
07749-0010000
Slide hammer weight
07741-0010201

1. Remove the ball bearing (A) from the clutch housing (B) using the 20−40 mm adjustable bearing puller (C), slide hammer weight (D) and bearing remover shaft (E).