( TL19E00J54200014401KDAT00 )

Battery Removal/Installation

NOTE: The battery terminal disconnection/reconnection procedure must be done before and after doing this procedure. Some systems store data in memory that is lost when the battery is disconnected.
Removal

1. Do the battery terminal disconnection procedure.

1. Remove the two nuts (A) securing the battery setting plate, then remove the battery setting plate (B), battery cover (C) and the battery (D).

Installation

1. Install the battery (A), then install the battery cover (B) and battery setting plate (C).

1. Tighten the two nuts (D) equally until the battery is stable.
   NOTE: Do not deform the battery setting plate by tightening the nuts too much.

1. Do the battery terminal reconnection procedure.
   NOTE: Make sure the positive terminal and the negative terminal are not reverse-connected.