( TL19E00J54300065801FHAT00 )

Wiper/Washer Switch Test/Replacement

1. Remove the steering column covers.

1. Disconnect the dashboard wire harness 8P connector (A) from the wiper/washer switch (B).

1. Remove the two screws, then slide out the wiper/washer switch.

1. Inspect the connector terminals to be sure they are all making good contact.
   - If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system.
   - If the terminals look OK, go to Step 5 .

LHD model, KE and KN models
KQ model