( TL19E00J46127053949KBAT00 )

Front Seat-back Cover Replacement

1. From under the seat cushion, disconnect and/or detach the connector(s):
   - Driver's seat:

   - | Side airbag connector (A)
   - | Recline motor harness connector (B) (8-way power seat)
   - | Seat-back heater connector (C) (8-way power seat/ some manual height adjustable seat)

   - Passenger's seat:

   - | Side airbag connector (A)
   - | Recline motor harness connector (B) (8-way power seat)
   - | Seat-back heater connector (C) (8-way power seat/ some manual seat without OPDS)

1. Detach the harness clips (E), and remove the harness clamps (F).

Driver's seat (8-way power seat)
Driver's seat (except 8-way power seat)
Passenger's seat without OPDS (8-way power seat)
Passenger's seat without OPDS (manual seat)
Passenger's seat with OPDS on RHD model (8-way power seat)
Passenger's seat with OPDS on RHD model (manual seat)