( TL19E00J46643420703FEAT00 )

Door Key Cylinder Switch Test

1. Remove the driver's door panel.

1. Disconnect the 10P connector from the key cylinder switch.

1. Check for continuity between the terminals.
   - There should be continuity between the No. 8 [No. 7] and No. 5 [No. 10] terminals when the door key cylinder switch is in UNLOCK position.
   - There should be no continuity between the No. 8 [No. 7] and No. 5 [No. 10] terminals when the door key cylinder switch is in the neutral or LOCK position.
   - There should be continuity between the No. 9 [No. 6] and No. 5 [No. 10] terminals when the door key cylinder switch is in LOCK position.
   - There should be no continuity between the No. 9 [No. 6] and No. 5 [No. 10] terminals when the door key cylinder switch is in the neutral or UNLOCK position.

   [ ]: | RHD model

1. If the continuity is not as specified, replace the door lock cylinder assembly.