( TL19E00B44100036401KBAT00 )

Rear Knuckle/Hub Bearing Unit Replacement

1. Remove the lock pin (A) from the upper arm ball joint, then remove the castle nut (B).
   NOTE: During installation, install the lock pin as shown after tightening the new castle nut.

1. Disconnect the upper arm ball joint from the knuckle using the ball joint remover.
   NOTE:
   - Be careful not to damage the boll joint boot when installing the remover.
   - During installation, to connect the ball joint, raise up the suspension with a jack.