( TL19E1AE34150719632KBAT00 )

M/T Differential Oil Seal Replacement

Special Tools Required
Driver handle, 15 x 135L
07749-0010000
Bearing driver attachment, 52 x 55 mm
07NAD-P200100

1. Remove the oil seal (A) from the transmission housing (B).
   NOTE: Be careful not to damage the transmission housing while removing the oil seals.

1. Remove the oil seal (A) from the clutch housing (B).

1. Install the new oil seal in the transmission housing with the 15 x 135L driver handle (A) and the 52 x 55 mm bearing driver attachment (B).

1. Install the new oil seal in the clutch housing with the 15 x 135L driver handle (A) and the 52 x 55 mm bearing driver attachment (B).