( TL19E20A18313200000LAAT00 )

Balancer Shaft/Balancer Shaft Holder Assembly Overhaul

1. Remove the upper balancer shaft holder and the bearings again, and measure the widest part with the plastigage.
   - If the front balancer shaft No. 1 journal and the rear balancer shaft No. 1, 2 journals oil clearance is out-of-tolerance, replace the balancer shaft and recheck. If it is still out-of-tolerance, replace the balancer shaft holders.
   - If the front balancer shaft No. 2 journal and the rear balancer shaft No. 3 journal oil clearance is out-of-tolerance, install new bearings, and recheck. If it is still out-of-tolerance, replace the balancer shafts.

   Journal Oil Clearance
   Front No. 1 Journal:
   Standard (New): | 0.030−0.062 mm (0.0012−0.0024 in.)
   Service Limit: | 0.08 mm (0.003 in.)
   Front No. 2 Journal:
   Standard (New): | 0.04−0.10 mm (0.002−0.004 in.)
   Service Limit: | 0.13 mm (0.005 in.)
   Rear No. 1, 2 Journals:
   Standard (New): | 0.030−0.062 mm (0.0012−0.0024 in.)
   Service Limit: | 0.08 mm (0.003 in.)
   Rear No. 3 Journal:
   Standard (New): | 0.04−0.10 mm (0.002−0.004 in.)
   Service Limit: | 0.13 mm (0.005 in.)