( TL19E00J18573437303KBAT00 )

Rear License Trim Replacement

NOTE:

- Take care not to scratch the trunk lid.
- When removing components, use the trim tools or equivalent.

1. Pull the rear license trim (A) out to detach the clips, then remove the trim.

1. Install the trim in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.