( TL19E00H46200053401KBAT00 )

Front Seat Belt Replacement

Front Seat Belt Buckle

1. Do the battery terminal disconnection procedure, then wait at least 3 minutes before beginning work.

1. Remove the front seat.

1. Lift up the front seat, then disconnect and/or detach the seat belt switch connecter (A), and detach the harness clip (B).
   NOTE: The front seats on LHD model are shown; the ones on RHD model are symmetrical.

Driver's seat (8-way power seat)
Driver's seat (manual seat/manual height adjustable seat without seat heater)
Driver's seat (manual height adjustable seat with seat heater)
Passenger's seat (8-way power seat)
Passenger's seat (manual seat without seat heater)
Passenger's seat (manual seat with seat heater)