( TL19E00J46127053949KBAT00 )

Front Seat-back Cover Replacement

1. Install the cover in the reverse order of removal, and note these items:
   - For some models: Reinitialize the OPDS unit.
   - To prevent wrinkles when installing a seat-back cover, make sure the material is stretched evenly over the pad before securing the upholstery rings, the hooks, and the hook strips.
   - Before installing the seat-back cover, make sure airbag wires (A, B) are installed to the reinforcing cloths (C) correctly.
   - Replace any upholstery rings you removed with new ones (D). Install them with commercially available upholstery ring pliers (E).
   - Reinstall airbag wire A, and B securely.
   - Use only original Honda replacement seat-back covers.
   - Make sure the side airbag harness and the OPDS unit harness (some passenger's seat) are routed properly.