( TL19E00J34600000000CAAT00 )

Auto Door Locks (Unlock) (KN model)
The driver's MICU controls the door lock actuators based upon the input signals from each switch.

| Input | Output
--- | --- | ---

Driver's MICU

IG1 power supply
Transmission range switch (P position)
Driver's door switch
Left [right] rear door switch
Trunk lid latch switch
Left [right] rear door lock knob switch (UNLOCK)

Driver's door lock actuators (UNLOCK)
Door lock actuators (UNLOCK)

B-CAN | Front passenger's door switch Right [left] rear door switch Driver's door lock knob switch (UNLOCK) Front passenger's door lock knob switch (UNLOCK) Right [left] rear door lock knob switch (UNLOCK) | Door lock (UNLOCK) signal

[ ]: | RHD model