( TL19E00J18526327895KBAT00 )

Fuel Fill Door Adapter Replacement

1. Install the adapter in the reverse order of removal, and note these items:
   - Before installing the grommet, clean the body bonding surface with isopropyl alcohl.
   - Install the grommet by pushing on the hook portions until the hooks snap into place, and push the seal portion to make the adhesive stick securely.
   - Apply multipurpose grease to the rod (A) sliding portion of the grommet (B).
   - Make sure the fuel fill door adapter is set the fuel filler pipe properly. Take care not to deform the packing of the adapter.
   - Apply medium strength liquid thread lock to the fuel filler pipe mounting bolts before reinstallation.