( TL19E1PE10410610101KBAT00 )

A/T 2nd Clutch Transmission Fluid Pressure Switch Replacement

1. Remove the intake air duct.

1. Disconnect the connector (A) from the 2nd clutch transmission fluid pressure switch (B), then remove the 2nd clutch transmission fluid pressure switch.

1. Install a new 2nd clutch transmission fluid pressure switch with a new sealing washer (C), and tighten the 2nd clutch transmission fluid pressure switch to the specified torque by turning the metal part, not the plastic part.

1. Check the connector for rust, dirt, or oil, and clean or repair if necessary, then connect the connector securely.

1. Install the intake air duct.