( TL19E00J54260462100CBAT00 )

Fuse to Components Index - Under-hood Fuse/Relay Box

Under-hood Fuse/Relay Box

Fuse Number | Amps | Component(s) or Circuit(s) Protected
--- | --- | ---
1 | MAIN | 100 A | Battery, Power supply
AS F/B | 60 A *1 | No. 7 to No. 13 fuses, No. 20 and No. 21 fuses (in the passenger's under-dash fuse/relay box)
40 A *2
2 | 2-1 | EPS | 70 A | EPS control unit
2-2 | AS F/B OP | 40 A | No. 14 to No. 22 fuses (in the passenger's under-dash fuse/relay box)
2-3 | VSA FSR | 30 A | VSA modulator-control unit (FSR)
2-4 | Not used | ——— | Not used
2-5 | VSA MTR | 30 A | VSA modulator-control unit (MTR)
2-6 | Not used | ——— | Not used
3 | 3-1 | IG MAIN | 50 A | No. 1 to No. 7 fuses and No. 9 to No. 13 fuses (in the driver's under-dash fuse/relay box)
3-2 | DR F/B | 40 A *4 | No. 14 fuse, No. 19 to No. 25 fuses (in the driver's under-dash fuse/relay box)
3-3 | AS LT MAIN | 50 A | No. 1 to No. 5 fuses (in the passenger's under-dash fuse/relay box)
3-4 | DR F/B | 60 A *3 | No. 14 fuse, No. 19 to No. 25 fuses (in the driver's under-dash fuse/relay box)
3-5 | DR LT MAIN | 40 A | No. 26 to No. 31 fuses (in the driver's under-dash fuse/relay box)
3-6 | MAIN FAN MTR | 30 A | Radiator fan motor (via radiator fan relay)
3-7 | Not used | ——— | Not used
3-8 | WIP MTR | 30 A | Wiper motor (high/low) (via wiper motor relay circuit in the relay circuit board)
4 | 40 A | Condensers (via rear window defogger relay), Rear window defogger (via rear window defogger relay)
5 | 20 A | A/C condenser fan motor (via A/C condenser fan relay circuit in the relay circuit board)
6 | ——— | Not used
7 | ——— | Not used
8 | 40 A | Blower motor (via blower motor relay)
9 | 15 A | Driver's MICU, Hazard warning switch (via driver's under-dash fuse/relay box)
10 | 10 A | Cruise control combination switch *1 , Distance switch *1 , Horns (high, low), Horn switch, Security horn relay

*1: | With ACC
*2: | Without ACC
*3: | With power seat or sunroof
*4: | Without power seat and sunroof

Under-hood Fuse/Relay Box

Fuse Number | Amps | Component(s) or Circuit(s) Protected
--- | --- | ---
11 | 30 A | Headlight washer relay *2 , Headlight washer motor *2
12 | 15 A | ACC unit *1 , Brake lights, Brake pedal position switch (via relay circuit board) *1 , VSA modulator-control unit
13 | 15 A | Ignition coils (No. 1 to No. 4) (via ignition coil relay)
14 | 15 A | A/F sensor (SENSOR1), ECM/PCM (SUBRLY)

15 (LHD model)

10 A

Via driver's under-dash fuse/relay box:
ACC unit *1 , Automatic lighting/rain sensor, Data link connector (DLC), Door multiplex control unit (power window master switch), Driver's door courtesy light, Driver's MICU, Front Passenger's door courtesy light, Gauge control module, Immobilizer-keyless control unit, Microphone (with navigation)
Via passenger's under-dash fuse/relay box:
Audio unit, Center display unit, Audio/navigation switch panel, Hands Free Telephone control unit, Navigation display unit, Navigation unit, Passenger's MICU, Power seat control unit (with DPMS)

15 (RHD model)

Via passenger's under-dash fuse/relay box:
ACC unit *1 , Audio unit (without navigation), Audio/navigation switch panel, Automatic lighting/rain sensor, Data link connector (DLC), Door multiplex control unit (power window master switch), Driver's door courtesy light, Front passenger's door courtesy light, Gauge control module, Hands Free Telephone control unit, Immobilizer-keyless control unit, Ultrasonic off switch, Ultrasonic/inclination sensor off switch, Microphone (with navigation), Navigation unit, Passenger's MICU, Power seat control unit (with DPMS)
Via driver's under-dash fuse/relay box:
Driver's MICU, Inclination sensor, Ultrasonic siren

16 (LHD model) | 7.5 A | Via driver's under-dash fuse/relay box: Ceiling light, Driver's vanity mirror light, Ignition key light, Left rear door courtesy light, Map lights, Passenger's vanity mirror light, Trunk light Via passenger's under-dash fuse/relay box: Right rear door courtesy light
16 (RHD model) | Via passenger's under-dash fuse/relay box: Ceiling light, Driver's vanity mirror light, Ignition key light, Left rear door courtesy light, Map light, Passenger's vanity mirror light Via driver's under-dash fuse/relay box: Right rear door courtesy light, Trunk light

17

15 A

CKP sensor, CMP sensor B, ECM/PCM (ETCSRLY) (via electronic throttle control system (ETCS) control relay), ECM/PCM (IGP), ECM/PCM (MRLY), Injectors (No. 1 to No. 4), MAF sensor, PGM-FI main relay 1 (FI MAIN)
Via driver's under-dash fuse/relay box:
ECM/PCM (IMOFPR)

18 | 15 A | ECM/PCM (IG1ETCS), Electronic throttle control system (ETCS) control relay
19 | ——— | Not used
20 | 7.5 A | A/C compressor clutch
21 | 7.5 A | ECM/PCM (via A/C condenser fan relay circuit in the relay circuit board)

*1: | With ACC
*2: | With headlight washer