( TL19E00J32373700000FHAT00 )

Trunk Light Test/Replacement

1. Open the trunk lid.

1. Carefully pry out the trunk light (A).

   Trunk Light: | 5 W

1. Disconnect the 2P connector (B) from the light.

1. Check for continuity between the No. 1 (+) and No. 2 (−) terminals. There should be continuity. If there is no continuity, check the bulb. If the bulb is OK, replace the trunk light assembly.

1. Install the light in the reverse order of removal.