( TL19E1PE10411354181MAAT00 )

A/T Secondary Shaft 2nd Gear Axial Clearance Inspection

1. Install the thrust needle bearing (A), the needle bearing (B), 2nd gear (C), the thrust needle bearing (D), the 37 x 58 mm thrust washer (E), and the 2nd clutch (F) on the secondary shaft (G), then secure them with the snap ring (H). Do not install the O-rings during inspection.

1. Measure the clearance between the snap ring (A) and the 2nd clutch guide (B) using a feeler gauge (C), in at least three places. Use the average as the actual clearance.

   Standard: | 0.04−0.12 mm (0.002−0.005 in.)

1. If the clearance is out of standard, remove the 37 x 58 mm thrust washer, and measure its thickness.

1. Select and install a new thrust washer, then recheck.
   THRUST WASHER, 37 x 58 mm

   No. | Part Number | Thickness
   --- | --- | ---
   1 | 90511-PRP-010 | 3.900 mm (0.154 in.)
   2 | 90512-PRP-010 | 3.925 mm (0.155 in.)
   3 | 90513-PRP-010 | 3.950 mm (0.156 in.)
   4 | 90514-PRP-010 | 3.975 mm (0.156 in.)
   5 | 90515-PRP-010 | 4.000 mm (0.157 in.)
   6 | 90516-PRP-010 | 4.025 mm (0.158 in.)
   7 | 90517-PRP-010 | 4.050 mm (0.159 in.)
   8 | 90518-PRP-010 | 4.075 mm (0.160 in.)
   9 | 90519-PRP-010 | 4.100 mm (0.161 in.)
   10 | 90520-PRP-010 | 4.125 mm (0.162 in.)
   11 | 90521-PRP-010 | 4.150 mm (0.163 in.)
   12 | 90522-PRP-010 | 4.175 mm (0.164 in.)
   13 | 90523-PRP-000 | 4.200 mm (0.165 in.)
   14 | 90524-PRP-000 | 4.225 mm (0.166 in.)
   15 | 90525-PRP-000 | 4.250 mm (0.167 in.)
   16 | 90526-PRP-000 | 4.275 mm (0.168 in.)
   17 | 90527-PRP-000 | 4.300 mm (0.169 in.)
   18 | 90528-PRP-000 | 4.325 mm (0.170 in.)
   19 | 90529-PRP-000 | 4.350 mm (0.171 in.)
   20 | 90530-PRP-000 | 4.375 mm (0.172 in.)

1. After replacing the thrust washer, make sure the clearance is within standard.

1. Disassemble the installed parts from the secondary shaft.