( TL19E1PE10410613041FHAT00 )

ATF Temperature Sensor Test/Replacement

1. Disconnect the connectors from the shift solenoid valves, and replace the ATF temperature sensor and the shift solenoid wire harness (F).

1. Install a new O-ring (G) on a new shift solenoid wire harness, then install the shift solenoid wire harness in the transmission housing. Secure the shift solenoid wire harness with the bolt.

1. Connect the shift solenoid wire harness terminal to the shift solenoid valves.
   - BLU wire connector to shift solenoid valve A.
   - ORN wire connector to shift solenoid valve B.
   - GRN wire connector to shift solenoid valve C.
   - YEL, WHT, and WHT wire connector to shift solenoid valve D.
   - RED wire connector to shift solenoid valve E.

1. Install a new gasket, the dowel pins, and the shift solenoid valve cover.

1. Install a new O-ring on the ATF dipstick guide tube, then install the guide tube. Secure the guide tube with the bolts.

1. Check the shift solenoid wire harness connector for rust, dirt, or oil, and clean if necessary, then connect the connector securely.

1. Secure the ATF cooler line with the bolts.

1. Install the harness clamps on the clamp brackets.

1. Install the battery base.

1. Install the air cleaner housing and the intake air duct.

1. Install the splash shield.

1. Install the left front wheel.

1. Do the battery installation procedure.
   NOTE: Do not the test-driving until Step 30 .

1. Refill the transmission with ATF.