( TL19E00J34200000000MAAT00 )

Sunroof Closing Force and Opening Drag Check

1. Opening drag check: Protect the leading edge of the glass with a shop towel (A). Measure the effort required to open the glass using a spring scale (B) as shown.

1. If the load is over 40 N (4 kgf, 9 lbf), check:
   - The side clearance and glass position adjustment.
   - For broken or damaged sliding parts. If any sliding parts are damaged, replace them.

1. Reset the sunroof control unit after reinstalling the sunroof motor.