( TL19E1PE10410917424KBAT00 )

Torque Converter Housing Countershaft Bearing Replacement

Special Tools Required
Adjustable bearing remover set
07JAC-PH80000
Driver handle 15 x 135L
07749-0010000
Bearing driver attachment 62 x 68 mm
07746-0010500

1. Remove the countershaft bearing using the adjustable bearing remover set.

1. Remove the ATF guide plate (A), and check it for wear and damage. If the guide plate is worn or damaged, replace it.

1. Install the ATF guide plate in the torque converter housing, and install a new countershaft bearing (B).

1. Install the countershaft bearing securely in the torque converter housing using the 15 x 135L driver handle and the 62 x 68 mm bearing driver attachment.

1. Make sure that the bearing outer race notch-cut (A) is installed at a height of 0−0.05 mm (0−0.002 in.) (B) above the torque converter housing surface (C). Do not install the countershaft bearing higher than 0.05 mm (0.002 in.) above the torque converter housing surface.