( TL19E00J54226561995KDAT00 )

Under-dash Fuse/Relay Box (Driver's MICU) Removal/Installation

Installation

1. Install the relays and connect the connectors to the driver's under-dash fuse/relay box, then install the driver's under-dash fuse/relay box in the reverse order of removal.

1. Install the removed parts in the reverse order of removal.

1. Do the battery terminal reconnection procedure steps 1 to 4.

1. Register the immobilizer system with the HDS.
   NOTE: The imoes unit is built into the driver's MICU which is part of the driver's under-dash fuse/relay box. Because of this construction, the imoes unit must be registered, or the vehicle will not start.

1. Do the remaining steps of battery terminal reconnection procedure.

1. Confirm that all systems work properly.