( TL19E00J36100000000CAAT20 )

Navigation Unit Inputs and Outputs
Navigation Unit Connector D (5P) (KG and KE models)

Terminal Number | Wire Color | Terminal Name | Description | Voltage (about) | Symptom
--- | --- | --- | --- | --- | ---
1 | RED | HFT COMM3 (HFT communication 3) | Communication signal for HFT | ——— | Solid red HFT icon in Navi System Link
2 | WHT | HFT COMM4 (HFT communication 4) | Communication signal for HFT | ——— | Solid red HFT icon in Navi System Link
3 | BLK | HFT COMM1 (HFT communication 1) | Communication signal for HFT | ——— | HFT icon in Navi System Link changes between red and green
4 | GRN | HFT COMM2 (HFT communication 2) | Communication signal for HFT | ——— | HFT icon in Navi System Link changes between red and green
5 | GRY * | HFT COMM SH (HFT communication shield) | Shield for terminals No.1, 2, 3, 4 | ——— | ———

*: | The shielded wires have a heat-shrink tube insulating the outside of the wire. The color of the insulating tube, typically black or dark gray, may not match the color of the wire shown on the circuit diagram.