( TL19E1AE34150400000MAAT00 )

M/T Mainshaft Assembly Clearance Inspection

1. Measure the clearance between 6th gear (A) and the angular ball bearing (B) with a feeler gauge (C). If the clearance is more than the service limit, go to Step 11 .
   R20A3 Engine Model:

   | Standard: | 0.06−0.16 mm (0.002−0.006 in.)
   | Service Limit: | 0.25 mm (0.010 in.)

   K24Z3 Engine Model:

   | Standard: | 0.15−0.25 mm (0.006−0.010 in.)
   | Service Limit: | 0.34 mm (0.013 in.)