( TL19E20A14400065101KBAT00 )

Water Pump Replacement

1. Drain the engine coolant.

1. Remove the drive belt auto-tensioner.

1. Remove the water pump (A) by removing the five bolts.

1. Inspect, and clean the O-ring groove and the mating surface of the engine block.

1. Install the water pump with a new O-ring (B) in the reverse order of removal.

1. Clean up any spilled engine coolant.

1. Install the drive belt auto-tensioner.

1. Refill the radiator with engine coolant, then bleed air from the cooling system.