( TL19E00F00000059501KBAT00 )

Steering Tie-rod Ball Joint Boot Replacement

1. Install the new tie-rod ball joint boot (A) using the inner bearing driver attachment. The boot must not have a gap at the boot installation sections (B). After installing the boot, check the ball pin tapered section for grease contamination, and wipe it if necessary.

1. Install the tie-rod end to the rack end.

1. Connect the tie-rod ball joint to the knuckle.

1. Check the wheel alignment, and adjust it if necessary.