( TL19E20A14680300000FAAT00 )

VTEC System Oil Pressure Troubleshooting

1. Connect the battery positive terminal (+) to terminal No. 1, and the negative terminal (−) with a wire.

1. Start the engine.

1. Check the oil pressure at the engine speed of 3,500 rpm (min −1 ).
   NOTE: Keep the measuring time as short as possible (less than 1 minute).

Is the oil pressure above 392 kPa (4.0 kgf/cm 2 , 56.9 psi)?

YES | - | Troubleshooting is complete.■
NO | - | Clean the oil passage of the cylinder block or replace the cylinder block.■