( TL19E00H46400012803KBAT00 )

Front Passenger's Airbag Replacement

1. Connect the dashboard wire harness 4P connector (A) to front passenger's airbag, then reinstall the glove box.

1. Do the battery terminal reconnection procedure.

1. Connect the HDS and clear the DTCs.

1. After installing the airbag, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.