( TL19E00J54460647105FEAT01 )

Power Window Rear Motor Test - With All Power Windows AUTO UP/DOWN Function

With all power windows AUTO UP/AUTO DOWN function
Motor Test

1. Remove the rear power window switch.

1. Test the motor in each direction by connecting battery power and ground to the rear power window switch 14P connector (A) according to the table.

1. If the motor does not run or fails to run smoothly, go to Step 4 .

1. Remove the door panel.

1. Disconnect the 6P connector (A) from the rear power window motor (B).

1. Check for continuity between the rear power window switch 14P connector No. 1 and No. 7 terminals and the rear power window motor 6P connector No. 1 and No. 4 terminals respectively. There should be continuity.

   REAR POWER WINDOWSWITCH 14P CONNECTOR | REAR POWER WINDOWMOTOR 6P CONNECTOR
   --- | ---
   No. 1 terminal | No. 1 terminal
   No. 7 terminal | No. 4 terminal

1. If the wire harness is OK, replace the rear power window motor.

Pulser Test

1. Do the rear power window switch input test No. 10, No. 11, and No. 12 terminals.