( TL19E00K73500000000BBAT10 )

How to Troubleshoot the HFT System

Pairing Your Cell Phone (A One Time Procedure)
NOTE:

- You cannot pair a phone if the vehicle is moving.
- Your phone must be in its Discovery mode.
- Up to six Bluetooth compatible phones can be paired by the HFT.

1. Turn on your phone, and follow the prompts to activate Bluetooth.

1. Give these voice commands to the HFT by pressing the talk button.

   You say | You'll hear
   --- | ---
   ‘‘Phone setup'' | ‘‘Phone setup options are status, pair, edit, delete, and list.''
   ‘‘Pair'' | ‘‘The pairing process requires operation of your mobile phone. For safety, only perform this function while the vehicle is stopped. State a four-digit code for pairing. Note this code, it will be requested by the phone.''
   ‘‘1. 2. 3. 4.'' (This can be any four-digit code you want.) | ‘‘1. 2. 3. 4. is this correct?''
   ‘‘Yes'' | ‘‘Searching for a Bluetooth phone. Make sure the phone you are trying to pair is in Discovery mode!''

1. Follow the cell phone manufacturer's instructions to put the phone in its Discovery mode. The phone will search for the HFT. When you see Hands Free Telephone in the device list on the phone, select it.

1. When prompted, enter the four-digit PIN from step 2 into the phone. You will hear the HFT say ‘‘A new phone has been found. Would you like to name this phone?''

1. Press and release the Talk button, and say what the phone name will be. For example, say ‘‘John's phone''. You'll hear ‘‘John's phone has been successfully paired'', returning to the main menu.

1. To pair another phone, repeat Step 1 thru 5.