( TL19E00J34600000000CAAT00 )

Power Door Lock (LOCK)
The driver's MICU controls the door lock actuators LOCK operation based upon the input signals of each switch.

| Input | Output
--- | --- | ---

Driver's MICU

IG1 power supply
Transmission range switch (P)
Driver's door switch
Left [right] rear door switch
Left [right] rear door lock knob switch (UNLOCK)
Brake pedal position switch Trunk lid latch switch

Door lock actuators (LOCK)

B-CAN

Front passenger's door switch
Right [left] rear door switch
Driver's door lock switch (UNLOCK)
Front passenger's door lock switch (UNLOCK)
Front passenger's door lock knob switch (UNLOCK)
Right [left] rear door lock knob switch (UNLOCK)
Vehicle speed signal

Door lock (LOCK) signal

[ ]: | RHD model