( TL19E00J18573430211KBAT00 )

Front Grille Cover Replacement

NOTE: Take care not to scratch the front grille and the body.

1. Remove the front grille cover (A).

   -1. | Remove the clips.
   -2. | Pass both hood edge cushions (B) through the holes in the cover by pulling the rear edge of the cover up, and slide the entire cover rearward to release it from the groove (C) of the front grille (D).
   -3. | Pass the hood latch knob (E) through the hole in the cover.

1. Install the cover in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.