( TL19E1AE34116317031LAAT00 )

Clutch Master Cylinder Overhaul

1. Remove the piston assembly (A), the connector (B), and the O-ring (C).

1. Apply the rubber grease to the piston, and slide the piston assembly into the clutch master cylinder, then install the pushrod with the stopper plate, and the circlip in the groove of the clutch master cylinder while pushing the piston.

1. Install the connector with a new O-ring.

1. Connect the clutch line connector and the reservoir hose to the master cylinder, then install the clutch master cylinder.