( TL19E1PE10410613041FHAT00 )

ATF Temperature Sensor Test/Replacement

1. Raise the vehicle on a lift, or apply the parking brake, block the rear wheels, and raise the front of the vehicle. Make sure it is securely supported.

1. Remove the left front wheel.

1. Remove the splash shield.

1. Remove the drain plug (A), and drain the transmission fluid (ATF).

1. Reinstall the drain plug with a new sealing washer (B).

1. Do the battery removal procedure.

1. Remove the battery base.

1. Remove the air cleaner housing and the intake air duct.