( TL19E00G10100050652KBAT00 )

A/C Refrigerant Oil Replacement

Recommended PAG oil: SP-10

- P/N 38897-P13-A01AH: 120 mL (4 fl·oz, 4.2 Imp·oz)
- P/N 38899-P13-A01: 40 mL (1 1/3 fl·oz, 1.4 Imp·oz)

Add the recommended refrigerant oil in the amount listed if you replace any of the following parts.

- To avoid contamination, do not return the oil to the container once dispensed, and never mix it with other refrigerant oils.
- Immediately after using the oil, reinstall the cap on the container, and seal it to avoid moisture absorption.
- Do not spill the refrigerant oil on the vehicle; it may damage the paint; if it gets on the paint, wash it off immediately.

A/C condenser (including Dryer Desiccant) . | 50 mL (1 2/3 fl·oz, 1.8 Imp·oz)
Evaporator . | 40 mL (1 1/3 fl·oz, 1.4 Imp·oz)
Line or hose . | 10 mL (1/3 fl·oz, 0.4 Imp·oz)
Receiver/Dryer Desiccant . | 10 mL (1/3 fl·oz, 0.4 Imp·oz)
Leakage repair . | 25 mL (5/6 fl·oz, 0.9 Imp·oz)
A/C compressor . | Since the oil separator is equipped inside the compressor for this vehicle, oil drainage is unnecessary at the time of compressor replacement.