( TL19E00J26273450001KDAT00 )

Interior Trim Removal/Installation - Rear Shelf Area

1. Remove the rear bulkhead cover (A).

   -1. | Remove the belt hole lid (B) by releasing the hooks (C).
   -2. | Gently pull back the front edge of the cover to detach the clips (D).
   -3. | Pull up the cover to detach the clips (E) fastening it to the body. and the clip (F) fastening it to the rear shelf (G).
   -4. | Lift the cover upward and forward to release each anchor rod (H) out through the hole in the cover.
   -5. | Pull both rear seat belts (I) and rear center seat belt (J) out through the slits (K) and the hole (L) in the cover.
   -6. | Carefully move the cover above the rear wheelhouse gussets (M), then remove it.