( TL19E00J18575360438FHAT00 )

Trunk Lid Outer Handle Switch Test/Replacement

1. Open the trunk lid, and remove the trunk lid trim.

1. Disconnect the 3P connector (A) from the trunk lid outer handle switch (B).

1. Check for continuity between the No. 2 and No. 3 terminal.
   - With the switch pushed, there should be continuity.
   - With the switch released, there should be no continuity.

1. If the continuity is not as specified, remove lock plate (C) and replace the switch.