( TL19E00K80100081610FAAT00 )

DTC Troubleshooting: 61, 62

DTC 61:
Low +B-FSR Voltage
DTC 62:
High +B-FSR Voltage
NOTE: If the vehicle has high electric load or a weak battery, DTC 61 may be stored when starting the engine.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0), then turn it to ON (II) again.

Does the ABS indicator come on?

YES | - | Go to Step 4 .
NO | - | The system is OK at this time.■

1. Check for DTCs with the HDS.

Is DTC 61 or 62 indicated?

YES | - | Check the battery and the charging system: R20A3 engine model, K24Z3 engine model. ■
NO | - | Do the appropriate troubleshooting for the DTC indicated.■