( TL19E00G24113600000KDAT00 )

Blower Unit Removal/Installation

1. Remove the passenger's dashboard undercover.

1. Remove the passenger's dashboard trim.

1. Remove the glove box.

1. Remove the passenger's dashboard center lower cover.

1. Remove the bolts (A) and the connector clips (B). Then cut the plastic cross brace (C) in the glove box opening with diagonal cutters in the area shown. Retain plastic cross brace to be reinstalled later.

1. Remove the self-tapping screws, and the passenger's heater duct (A).

1. Disconnect the connector (A) from the blower motor and the wire harness clip (B).

1. LHD model: Remove the connector clip (A) and harness clip (B).

1. Disconnect the connector (C) from the recirculation control motor. Remove the self-tapping screws, the bolt, the mounting nuts, and the blower unit (D).

1. Install the unit in the reverse order of removal. Make sure that there is no air leakage.