( TL19E00J18533232201KBAT00 )

Hood Seal Replacement

NOTE: Take care not to scratch the front grille.

1. Remove these items:
   - Front grille cover
   - Front bumper
   - Front grille

1. Remove the front grille molding A from the front grille base.

1. Remove the hood center seal (B) from the front grille molding A by releasing the seal from the projections (C) of the molding.

1. Install the seal in the reverse order of removal.